(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 57)
    (zones 0)
    (modules 14)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad15)")
  (net 3 "Net-(A1-Pad14)")
  (net 4 "Net-(A1-Pad13)")
  (net 5 "Net-(A1-Pad12)")
  (net 6 "Net-(A1-Pad11)")
  (net 7 "Net-(A1-Pad10)")
  (net 8 "Net-(A1-Pad9)")
  (net 9 FutureLCD2)
  (net 10 FutureLCD)
  (net 11 VoltageDiv2)
  (net 12 VoltageDiv1)
  (net 13 GND)
  (net 14 "Net-(A1-Pad3)")
  (net 15 VCC)
  (net 16 "Net-(A1-Pad1)")
  (net 17 "Net-(A1-Pad28)")
  (net 18 "Net-(A1-Pad27)")
  (net 19 "Net-(A1-Pad26)")
  (net 20 Blue2)
  (net 21 Green2)
  (net 22 Red2)
  (net 23 Blue1)
  (net 24 Green1)
  (net 25 Red1)
  (net 26 "Net-(A1-Pad18)")
  (net 27 "Net-(A1-Pad17)")
  (net 28 "Net-(D1-Pad1)")
  (net 29 "Net-(D1-Pad4)")
  (net 30 "Net-(D1-Pad3)")
  (net 31 "Net-(D2-Pad3)")
  (net 32 "Net-(D2-Pad4)")
  (net 33 "Net-(D2-Pad1)")
  (net 34 "Net-(A1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Blue1)
    (add_net Blue2)
    (add_net FutureLCD)
    (add_net FutureLCD2)
    (add_net GND)
    (add_net Green1)
    (add_net Green2)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net Red1)
    (add_net Red2)
    (add_net VCC)
    (add_net VoltageDiv1)
    (add_net VoltageDiv2)
  )
  (module Module:Adafruit_Feather (layer B.Cu) (tedit 62389282)
    (at 127.490001 77.745001)
    (descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
    (tags "Adafruit Feather")
    (fp_text reference A1 (at 10.16 7.62) (layer B.SilkS))
    (fp_text value Adafruit_Feather_HUZZAH32_ESP32 (at 10.16 -45.72 -180) (layer B.Fab))
    (fp_text user %R (at 10.16 -19.05 -180) (layer B.Fab))
    (pad 16 thru_hole circle (at 0 -38.1 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 15 thru_hole circle (at 0 -35.56 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 14 thru_hole circle (at 0 -33.02 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad14)"))
    (pad 13 thru_hole circle (at 0 -30.48 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad13)"))
    (pad 12 thru_hole circle (at 0 -27.94 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad12)"))
    (pad 11 thru_hole circle (at 0 -25.4 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad11)"))
    (pad 10 thru_hole circle (at 0 -22.86 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad10)"))
    (pad 9 thru_hole circle (at 0 -20.32 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad9)"))
    (pad 8 thru_hole circle (at 0 -17.78 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 34 "Net-(A1-Pad8)"))
    (pad 7 thru_hole circle (at 0 -15.24 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 FutureLCD2))
    (pad 6 thru_hole circle (at 0 -12.7 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 FutureLCD))
    (pad 5 thru_hole circle (at 0 -10.16 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 11 VoltageDiv2))
    (pad 4 thru_hole circle (at 0 -7.62 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 15 VCC))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad1)"))
    (pad 28 thru_hole circle (at 20.32 -10.16 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad28)"))
    (pad 27 thru_hole circle (at 20.32 -12.7 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad27)"))
    (pad 26 thru_hole circle (at 20.32 -15.24 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad26)"))
    (pad 25 thru_hole circle (at 20.32 -17.78 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 12 VoltageDiv1))
    (pad 24 thru_hole circle (at 20.32 -20.32 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 20 Blue2))
    (pad 23 thru_hole circle (at 20.32 -22.86 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 21 Green2))
    (pad 22 thru_hole circle (at 20.32 -25.4 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 22 Red2))
    (pad 21 thru_hole circle (at 20.32 -27.94 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 23 Blue1))
    (pad 20 thru_hole circle (at 20.32 -30.48 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 24 Green1))
    (pad 19 thru_hole circle (at 20.32 -33.02 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 25 Red1))
    (pad 18 thru_hole circle (at 20.32 -35.56 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad18)"))
    (pad 17 thru_hole circle (at 20.32 -38.1 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad17)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Adafruit_Feather.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_RGB_Cree_CLV1A-FKB_3.2x2.8mm (layer F.Cu) (tedit 5EC67E92)
    (at 132.56 44.97)
    (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
    (tags "LED 3227")
    (attr smd)
    (fp_text reference D1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value LED_RGB_CLV1A-FKB (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.75 0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 4 smd rect (at 1.75 -0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 1.75 0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_RGB_Cree_CLV1A-FKB_3.2x2.8mm (layer F.Cu) (tedit 5EC67E92)
    (at 132.56 57.67)
    (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
    (tags "LED 3227")
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value LED_RGB_CLV1A-FKB (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 3 smd rect (at 1.75 0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at 1.75 -0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D2-Pad4)"))
    (pad 2 smd rect (at -1.75 0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 1 smd rect (at -1.75 -0.75 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 142.24 67.85 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 VoltageDiv1))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 134.62 67.85 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 VoltageDiv2))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 41.91)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 Red1))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 44.45)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 Green1))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 46.99)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 Blue1))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad3)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 54.61)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 Red2))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 57.15)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 Green2))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D2-Pad4)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 140.24 59.69)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 Blue2))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 142.24 76.74 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference TH1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value Thermistor_NTC (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 1.314999 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 VoltageDiv1))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 130.8862 69.945 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x02_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 608518ED)
    (at 135.89 78.4352 270)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J1 (at -1.524 -2.54 270) (layer F.SilkS))
    (fp_text value Conn_Header_JST_PH_1x02_P2mm_Vertical_SMD (at 0 5.715 90) (layer F.Fab))
    (fp_text user %R (at 2.6 1.2) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 VoltageDiv2))
    (pad 2 smd rect (at 0 2.54 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x02_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 125.73 83.82) (end 125.73 33.02) (layer Edge.Cuts) (width 0.9))
  (gr_line (start 149.86 83.82) (end 125.73 83.82) (layer Edge.Cuts) (width 0.9))
  (gr_line (start 149.86 33.02) (end 149.86 83.82) (layer Edge.Cuts) (width 0.9))
  (gr_line (start 125.73 33.02) (end 149.86 33.02) (layer Edge.Cuts) (width 0.9))
)
